**Hydraulic Shears**

**Lot 1 – Portable/Mobile Cutting Operations – Metal shears**

**Technical Specifications**

* 110v/240v Compatible
* Automatic shutoff
* Can be moved freely- castor wheels/lockable.
* Safety Cage around blade
* Movable foot pedal
* Electric/diesel engine option
* Automatic hold down clamps
* Blade 6’’- 12.5’’ inch
* Cutting capacity from 42mm- 63mm, 1.65’’- 2.5″ inch mild steel round bar.
* Extension cable options

**Lot 2 – Static Cutting Operations – Metal Shears**

**Technical Specifications**

* 110v/240v Compatible
* Automatic shutoff
* Can be moved freely- castor wheels/lockable.
* Safety Cage around blade
* Movable foot pedal
* Automatic hold down clamps
* Electric/diesel engine option
* Blade minimum 10.5’’ inch
* Cutting capacity from 42mm - 88mm, 1.65’’- 3.5″ inch mild steel round bar
* Feed in Stands/Conveyer option
* Extension cable options
* Safety Curtains or similar safety feature

We require individual unit prices of all equipment including other ancillary/spares pack for all machines that is put forward for consideration.